
Procedure SetFreq;Assembler;
ASM
mov dx, 03D4h
mov al, 011h
out dx,al 
mov dx, 03D5h
in al,dx 
and al, 07Fh
out dx,al
mov dx, 03C2h
mov al, 063h
out dx,al
mov dx, 03D4h
mov al, 00h
out dx,al 
mov dx, 03D5h
mov al, 060h
out dx,al
mov dx, 03D4h
mov al, 01h
out dx,al 
mov dx, 03D5h
mov al, 04Fh
out dx,al
mov dx, 03D4h
mov al, 02h
out dx,al 
mov dx, 03D5h
mov al, 050h
out dx,al
mov dx, 03D4h
mov al, 03h
out dx,al 
mov dx, 03D5h
mov al, 082h
out dx,al
mov dx, 03D4h
mov al, 04h
out dx,al 
mov dx, 03D5h
mov al, 054h
out dx,al
mov dx, 03D4h
mov al, 05h
out dx,al 
mov dx, 03D5h
mov al, 080h
out dx,al
mov dx, 03D4h
mov al, 06h
out dx,al 
mov dx, 03D5h
mov al, 0Ah
out dx,al
mov dx, 03D4h
mov al, 07h
out dx,al 
mov dx, 03D5h
mov al, 03Eh
out dx,al
mov dx, 03D4h
mov al, 08h
out dx,al 
mov dx, 03D5h
mov al, 00h
out dx,al
mov dx, 03D4h
mov al, 09h
out dx,al 
mov dx, 03D5h
mov al, 041h
out dx,al
mov dx, 03D4h
mov al, 010h
out dx,al 
mov dx, 03D5h
mov al, 0BAh
out dx,al
mov dx, 03D4h
mov al, 011h
out dx,al 
mov dx, 03D5h
mov al, 08Ch
out dx,al
mov dx, 03D4h
mov al, 012h
out dx,al 
mov dx, 03D5h
mov al, 08Fh
out dx,al
mov dx, 03D4h
mov al, 013h
out dx,al 
mov dx, 03D5h
mov al, 028h
out dx,al
mov dx, 03D4h
mov al, 014h
out dx,al 
mov dx, 03D5h
mov al, 040h
out dx,al
mov dx, 03D4h
mov al, 015h
out dx,al 
mov dx, 03D5h
mov al, 090h
out dx,al
mov dx, 03D4h
mov al, 016h
out dx,al 
mov dx, 03D5h
mov al, 08h
out dx,al
mov dx, 03D4h
mov al, 017h
out dx,al 
mov dx, 03D5h
mov al, 0A3h
out dx,al
mov dx, 03C4h
mov al, 01h
out dx,al 
mov dx, 03C5h
mov al, 01h
out dx,al
mov dx, 03C4h
mov al, 03h
out dx,al 
mov dx, 03C5h
mov al, 00h
out dx,al
mov dx, 03C4h
mov al, 04h
out dx,al 
mov dx, 03C5h
mov al, 0Eh
out dx,al
mov dx, 03CEh
mov al, 05h
out dx,al 
mov dx, 03CFh
mov al, 040h
out dx,al
mov dx, 03CEh
mov al, 06h
out dx,al 
mov dx, 03CFh
mov al, 05h
out dx,al
END;
