                                 Arkos presents
                                 
                                    Twither
                               
                       a 256 bytes intro at Forever 2009
                        Coded by Grim/Arkos^Semilanceata


               The intro will run on 64Kb+ RAM Amstrad CPC/Plus.

            Two executables are provided, if one fail then it's most
            likely a CRTC timing problem.   Try again with the other
            executable. If it fail too...  you own a CPC with a CRTC
            type 2, kthxbye.

            The source-code should be available at www.grimware.org

             The 256 bytes twister contest is over, Amstrad wins :)
            
            READY
            RUN"TWITHER

_______________________________ Colors tweaking ________________________________

            If you wanna play with the color-palette, read this.

            Disable the set ink in the intro:
             MEMORY &9FFF:LOAD"TWITHER.BIN":POKE &A010,2

            Choose your favorite flashy colors:
             BORDER <0-26>:INK 0,<0-26>:INK 1,<0-16>

            Call the intro manually
             MODE 2:CALL&A008
________________________________________________________________________________
                                        
